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BALLAST REGULATOR PRESTART CHECKLIST
CHECKLIST


	 DETAILS 

	Location
	
	Day/Night
	

	Plant No
	
	Make and Model
	

	Supervisors Name 
	


	PRE START ITEMS TO BE CHECKED DAILY
	MON
	TUE
	WED
	THU
	FRI
	SAT
	SUN

	Hour-meter Reading
	
	
	
	
	
	
	

	Walk around inspection [oil / water leaks, loose bolts, nuts, connections.]
	
	
	
	
	
	
	

	No evidence of hose or fitting deterioration, cracking, corrosion, wear, damage or mechanical abrasion on hydraulic or fuel systems?
	
	
	
	
	
	
	

	Engine oil level - top up as required
	
	
	
	
	
	
	

	Radiator coolant level - top up as required
	
	
	
	
	
	
	

	Engine belts - A/C, alt, fan, compressor
	
	
	
	
	
	
	

	Fuel level - top up as required / Drain water sediment bowl
	
	
	
	
	
	
	

	Hydraulic oil level - top up as required
	
	
	
	
	
	
	

	Transmission oil level
	
	
	
	
	
	
	

	Clean engine air filter
	
	
	
	
	
	
	

	Electrical -operation of lights, horn, gauges, reverse alarm, beacon, overloading warning device, alarms and shutdowns, air conditioner.
	
	
	
	
	
	
	

	Grease front plow, side plow and broom box guide columns
	
	
	
	
	
	
	

	Grease broom drum bearings, Broom tuff condition (replace if necessary)
	
	
	
	
	
	
	

	Operation of the dust suppression unit (if applicable)
	
	
	
	
	
	
	

	Rail sweep adjustment / condition (adjust / replace if necessary)
	
	
	
	
	
	
	

	Guards are in place, secure and good condition
	
	
	
	
	
	
	

	Machine functions, test all motions. 
	
	
	
	
	
	
	

	Warning signals, flags, torch, first aid kit, fire extinguisher, PPE.
	
	
	
	
	
	
	

	Rail wheels: visual inspection looking for flange damage, flat spots, cracks & overheating
	
	
	
	
	
	
	

	Inspect brake shoes for wear and condition
	
	
	
	
	
	
	

	Brake shoes correctly adjusted (as per operator’s manual)
	
	
	
	
	
	
	

	Clean windows and mirrors
	
	
	
	
	
	
	

	Drain water from air tanks
	
	
	
	
	
	
	

	Service and park brake operation
	
	
	
	
	
	
	


	LIST ANY DEFECTS
	DAY
	REPORTED  TO
	CLEARED  BY
	DATE

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	IMPORTANT NOTE:
If defect is a safety hazard or requires Immediate repair: PARK UP MACHINE, attach an

OUT of SERVICE tag, contact Supervisor and do not use, until repaired or cleared by Supervisor for use.

	Comments

	

	

	

	

	

	

	NEXT SERVICE DUE at:


  Hours

	
	Full Name
	Signature

	Monday checks performed by:  
	
	

	Tuesday checks performed by:  
	
	

	Wednesday checks performed by: 
	
	

	Thursday checks performed by: 
	
	

	Friday checks performed by:  
	
	

	Saturday checks performed by:  
	
	

	Sunday checks performed by: 
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