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	PERMIT TO SPRAY SEAL
Template


This template is to be used by the project team to ensure that environmental risks associated with spray sealing activities are effectively managed.
[bookmark: _Toc529870108]Steps in obtaining approval 
Fill in the Table below and send to your Project Environmental (Planning) Manager (EM) for review a minimum of 3 days prior to proposed sealing activities. 
The EM will review the environmental documents to determine compliance with the requirements and the approval authority to proceed.
Allow sufficient time in your project planning for the assessment/design and implementation of controls. Your EM will advise you of the anticipated turnaround times.
No works can commence outside of project boundaries until a documented approval has been received. 
[bookmark: _Toc529870109]
	1. ACTIVITY DETAILS 

	Approved Project:
	

	Permit number:
	

	Location / Chainage
	
(*Attach drawings of proposed location)

	Proposed activity date
	

	OOHW 
	Are works within normal construction hours?
☐ Yes   ☐ No
If no, OOHW permit is required.

	Scope of work
	

	Total area to be sealed
	



	2. PRE-PLANNING FOR ACTIVITY READINESS

	BOM Forecast checked within 24 hours of proposed works?
	☐ Not ≥50% chance of ≥5mm rainfall in 24 hrs after the activity
Real-time monitoring assigned/arranged (BOM radar + visual check)   
☐ Yes   ☐ No

	Curing Time Documentation

	Anticipated curing time based on material type/climatic conditions recorded:
 _______ hours (attach calculation record)
Environmental controls to remain in place for minimum 24 hrs post-application   ☐ Documented on a drawing/ECP and agreed

	Site Readiness
	Aggregate stockpiles located ≥50m from waterways / wet areas  
 ☐ Yes   ☐ No (if No, bund ≥300mm in place)


	
	Stockpiles bunded/contained to prevent run-on/runoff   ☐ Yes
Dust suppression measures available ☐ Yes
Spill kits available and stocked   ☐ Yes

	1. ENVIRONMETNAL CONTROLS REIVEW

	
	Drains in spray area covered   ☐ Yes

	
	Hydrocarbon booms installed at:
   ☐ Stormwater drains in catchment
   ☐ Waterways downstream

	
	ESCs in place (sediment socks, sandbags, bunds, etc.)   ☐ Yes
Sensitive areas protected (waterways, heritage sites, EECs)   ☐ Yes
Plan for managing/testing/treating ponded water prior to discharge   ☐ Yes

	2. 	APPLICATION CONTROLS 

	
	Aggregate placement plan confirmed:
☐ Pre-coated aggregate will be applied and rolled immediately after spraying

	
	Provision for water contained on alignment until seal cured   ☐ Yes

	
	Bridge Deck Works (if part of the scope of this activity):
   ☐ Drain points blocked
   ☐ Water diverted to single control point
   ☐ Hydrocarbon booms available on deck



	[bookmark: _Toc490051308]3.	AUTHOR CERTIFICATION  


	Permit Holder: 
	Signature: 


	Certification date: 


	Environmental Representative:
	Signature: 


	Certification date: 





	4. 	APPROVAL TO COMMENCE SEALING


	Construction Manager: 


	Signature: 

	Approval date: 




	6.	Permit Closure

	I confirm that all work for which this Permit was issued has been completed.

	Permit Holder:
	


	Signature:
	
	Date and time:
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