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	PROJECT & INSPECTION DETAILS

	Project:
	
	Subcontractor:
	

	Work Location:
	
	Pump ID:
	

	Inspection Completed By:
	

	Work Commencement Date:
	dd/mm/yy
	Work Commencement Time:
	XX:XX am/pm





	ITEM
	CHECK
	Please tick ()

	
	
	YES
	NO
	N/A

	1. 
	PLANT INDUCTION

	1.1
	Has the mobile concrete boom pump been successfully inducted onto the Project?
	
	
	

	1.2
	Has the operator provided the latest records? (service history, maintenance records)?
	
	
	

	2. 
	NON-DESTRUCTIVE TESTING (NDT) 

	2.1
	Wall thickness Non-Destructive Testing (NDT) has been completed on all critical components?
· Single wall or Twin wall (unverified manufacturer) - Monthly; or
· Twin wall (verified manufacturer) – 12 monthly
	
	
	

	3. 
	COMPETENCY RECORDS

	3.1
	Does the operator hold a valid High-Risk Work Licence (PB - Concrete Placing Boom) and Valid VOC? 
	
	
	

	3.2
	Has a plant pre-start been completed, confirming all safety devices and warnings (e-stop, hopper grates, interlocks, decals) are working and in good condition?
	
	
	

	4. 
	EQUIPMENT SETUP & GROUND CONDITIONS

	4.1
	Have ground conditions been assessed for stability, including verification of underground services and weight-bearing capacity?
	
	
	

	4.2
	Are outriggers fully extended and correctly supported with sole boards or dunnage outlined within Original Equipment Manufacturers (OEM) specifications?
	
	
	

	4.3
	Has an exclusion zone been established around the pump setup area, ensuring safe distances from workers, plant, and structures?
	
	
	

	4.4
	Is the pump set up within its rated working radius, ensuring no excessive reach beyond OEM specifications?
	
	
	

	5. 
	CONCRETE DELIVERY AND PUMP OPERATION

	5.1
	Concrete delivery trucks have approved/designated routes with a clear path to the hopper maintained?
	
	
	

	5.2
	A communication system is in place between the pump operator and hose hand?
	
	
	

	6. 
	HOSE WHIP AND BLOCKAGE PREVENTION

	6.1
	Are flexible hoses on the boom securely retained with a safety chain, sling, or other retaining device?
	
	
	

	6.2
	Are all pipe clamps and whip checks in place?
	
	
	





	7. 
	WASHOUT & CLEANING

	7.1
	Has a designated washout area been set up for concrete residue disposal?
	
	
	

	7.2
	Whip Chain/Line Restraint in place to enable safe blow-out process?
	
	
	

	7.3
	Have line-clearing been planned to ensure safe discharge of remaining concrete from the system?
	
	
	

	7.4
	Has sufficient concrete wash-out bags been provided?
	
	
	



	SIGN-OFF

		Authorised Engineer / Supervisor Name:
	
	Date:
	

	Concrete Pump Operator Name:
	
	Date:
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